/**
  @page Binary Description of the binary template
  
  @verbatim
  ******************** (C) COPYRIGHT 2014 STMicroelectronics *******************
  * @file    USB_Device/DFU_Standalone/Binary/readme.txt 
  * @author  MCD Application Team
  * @version V1.0.0
  * @date    18-June-2014
  * @brief   Description of the binary template example.
  ******************************************************************************
  *
  * Licensed under MCD-ST Liberty SW License Agreement V2, (the "License");
  * You may not use this file except in compliance with the License.
  * You may obtain a copy of the License at:
  *
  *        http://www.st.com/software_license_agreement_liberty_v2
  *
  * Unless required by applicable law or agreed to in writing, software 
  * distributed under the License is distributed on an "AS IS" BASIS, 
  * WITHOUT WARRANTIES OR CONDITIONS OF ANY KIND, either express or implied.
  * See the License for the specific language governing permissions and
  * limitations under the License.
  *
  ******************************************************************************
  @endverbatim

@par Example Description 

This directory contains a binary template (in DFU format) to be loaded into Flash memory using Device 
Firmware Upgrade application. This file was converted to the DFU format using the "DFU File Manager Tool"
included in the "DfuSe" PC software install.
For more details on how to convert a .bin file to DFU format please refer to the UM0412 user manual 
"Getting started with DfuSe USB device firmware upgrade STMicroelectronics extension" available from the
STMicroelectronics microcontroller website www.st.com.
   
This binary is a simple LED toggling. The LED3/LED4 toggles for a period of 100 ms.
The system Timer (Systick) is used for to generate the delay.
The offset address of this binary is 0x08007000 which matches the definition in DFU application
"USBD_DFU_APP_DEFAULT_ADD".


@par Hardware and Software environment

  - This example runs on STM32L051xx, STM32L052xx, STM32L053xx STM32L062xx and 
    STM32L063xx device lines RevZ.
    
  - This example has been tested with STM32L0538-DISCO board and can be
    easily tailored to any other supported device and development board.  

 * <h3><center>&copy; COPYRIGHT STMicroelectronics</center></h3>
 */
